How to run the DCT and IDCT examples ?

The following argument as the input to the PLX SystemC Platform

[-log:systemc.log ..\..\Implementation\ASM_Scheduler\Version2\assembled_files\Dynload.bin@SDRAM:0 ..\..\Applications\DCT\Final_Binary_code\kernel_dct.bin@EXTSRAM:0 ..\..\Applications\DCT\Final_Binary_code\kernel_dct_data.out@EXTSRAM:0x4B000 ..\..\Applications\IDCT\Final_Binary_code\kernel_idct.bin@EXTSRAM:0x70810 ..\..\Applications\IDCT\Final_Binary_code\kernel_idct_data.out@EXTSRAM:0xBB810]


-------------------------------------------------
Now, the dynamical loading which support five task can be loaded dynamically.
Five task load address shown as follows:
text[1~5] mean that the address in which the binary file of text to be loaded.
info[1~5] mean that the address in which the binary file of data to be loaded.

--task1--
text1 load address=> @EXTSRAM:0
info1 load address=> @EXTSRAM:0x4B000

--task2--
text2 load address=> @EXTSRAM:0x70810
info2 load address=> @EXTSRAM:0xBB810

--task3--
text3 load address=> @EXTSRAM:0xE1020
info3 load address=> @EXTSRAM:0x12C020

--task4--
text4 load address=> @EXTSRAM:0x151830
info4 load address=> @EXTSRAM:0x19C830

--task5--
text5 load address=> @EXTSRAM:0x1C2040
info5 load address=> @EXTSRAM:0x20D040

-------------------------------------------------
